IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "Option [Drawing Scale: 50.000000]"
Description: "Option [Global Unique Identifiers (GUID): Keep existing]"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Entire Model]"
Description: "Option [IFC Domain: All]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and ArchiCAD 2D elements: Off]"
Description: "Option [Convert 2D symbols of Doors and Windows: Off]"
Description: "Option [Explode Composite and Complex Profile elements into parts: Off]"
Description: "Option [Export geometries that Participates in Collision Detection only: On]"
Description: "Option [Multi-skin complex geometries: Building element parts]"
Description: "Option [Elements in Solid Element Operations: Extruded/revolved]"
Description: "Option [Elements with junctions: Extruded/revolved without junctions]"
Description: "Option [Slabs with slanted edge(s): Extruded]"
File name: "C:\Users\Maggioni\Desktop\RD_Mader.ifc"
Time stamp: "2017-09-11T08:19:19"
Author: "Architect"
Organization: "Building Designer Office"
Preprocessor: "PreProc - EDM 5.0"
Originating system: "IFC file generated by Graphisoft ArchiCAD-64 18.0.0 CZE FULL Windows version (IFC2x3 add-on version: 4020 CZE FULL)."
Authorization: "The authorising person"
Application: "ArchiCAD-64" version "18.0.0" identifier "IFC2x3 add-on version: 4020 CZE FULL" by Organization "Graphisoft" id "GS" description "Graphisoft"

People and organizations
  Person "Nedefinováno" of Organization "Nedefinováno"
  Owner history of Person "Nedefinováno" of Organization "Nedefinováno" | application "ArchiCAD-64" version "18.0.0" identifier "IFC2x3 add-on version: 4020 CZE FULL" by Organization "Graphisoft" id "GS" description "Graphisoft" | change ADDED | created 1505110758 (2017-09-11T06:19:18Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  CURRENCY: CZK
  TIMEUNIT: Year (conversion based)
  MASSUNIT: GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Projekt"
  IFCSITE "Exteriér" | latitude 41° 53′ 0″ | longitude 12° 30′ 0″ | elevation above sea level 0.
    IFCBUILDING "Budova"
      IFCBUILDINGSTOREY "Prizemie" | elevation 0.
        contains 33 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "stena 1 0807459005 250" | names: "MURO - 289", "MURO - 291", "MURO - 290" (+1 more) | material: layers "stena 1 0807459005" ("Gesso 333567147" 10., "Retino vuoto 2405621226" 150., "Gesso 334354855" 10., "Isolamento Styrofoam SM 360458039" 80.) | property sets: AC_Pset_RenovationAndPhasing
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Okno 18" | names: "FINESTRA - 482", "FINESTRA - 483" | material: materials ("Sfondo", "Intercapedine", "Sfondo", "Sfondo", "Sfondo", "Isolamento termico", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Intercapedine", "Sfondo", "Isolamento acustico") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Okno 18" | names: "FINESTRA - 482" | material: materials ("Sfondo", "Intercapedine", "Sfondo", "Sfondo", "Sfondo", "Isolamento termico", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Intercapedine", "Sfondo", "Isolamento acustico") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Ingresso a 1 Anta 12" | names: "PORTA - 279" | material: materials ("Sfondo", "Intercapedine", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo") | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Retino vuoto 3157531607 150" | FLOOR | names: "SOLAIO - 239" | material: layers "Retino vuoto 3157531607 150" ("Retino vuoto 3157531607" 150.) | property sets: AC_Pset_RenovationAndPhasing
          13 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Cartongesso 110 0598480581 100" | names: "MURO - 299", "MURO - 302", "MURO - 298" (+10 more) | material: layers "Cartongesso 110 0598480581" ("Gesso 4040786529" 10., "Intercapedine 334091939" 80., "Gesso 4040786529" 10.) | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Minimal space 2632848274 220" | FLOOR | names: "SOLAIO - 257" | material: layers "Minimal space 2632848274 220" ("Minimal space 2632848274" 220.) | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "stena 3 0598480581 170" | names: "MURO - 306" | material: layers "stena 3 0598480581" ("Gesso 333567147" 10., "Retino vuoto 2405621226" 150., "Gesso 334354855" 10.) | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Okno 18" | names: "FINESTRA - 484" | material: materials ("Sfondo", "Intercapedine", "Sfondo", "Sfondo", "Sfondo", "Isolamento termico", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Intercapedine", "Sfondo", "Isolamento acustico") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "2 Ante 12" | names: "FINESTRA - 485" | material: materials ("Sfondo", "Intercapedine", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Minimal space 2632848274 250" | FLOOR | names: "SOLAIO - 258" | material: layers "Minimal space 2632848274 250" ("Minimal space 2632848274" 250.) | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Dvoukøídlé okno 1 18" | names: "FINESTRA - 481" | material: materials ("Sfondo", "Intercapedine", "Sfondo", "Sfondo", "Sfondo", "Isolamento termico", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Intercapedine", "Sfondo", "Isolamento acustico") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          3 x IFCDOOR | type IFCDOORSTYLE "1A 12" | names: "PORTA - 280", "PORTA - 281" | material: materials ("Sfondo", "Intercapedine", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo") | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "1A Scorrevole Esterna 12" | names: "PORTA - 284" | material: materials ("Intercapedine", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo") | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "1A 12" | names: "PORTA - 283" | material: materials ("Sfondo", "Intercapedine", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo", "Sfondo") | property sets: Pset_DoorCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
      IFCBUILDINGSTOREY "Rez/pohlady 2D" | elevation 2450.
        contains 2 elements
          2 x IFCSLAB | type IFCSLABTYPE "Muratura 1695224766 250" | ROOF | names: "FALDA - 138" | material: layers "Muratura 1695224766 250" ("Muratura 1695224766" 250.) | property sets: AC_Pset_RenovationAndPhasing

Types
  IFCWALLTYPE "stena 1 0807459005 250" | 4 occurrences
  IFCWINDOWSTYLE "Okno 18" | SINGLE_PANEL | 2 occurrences | property sets: Vlastnosti èar okna, Vlastnosti okenního køídla - køídlo1
  IFCWINDOWSTYLE "Okno 18" | SINGLE_PANEL | 1 occurrence | property sets: Vlastnosti èar okna, Vlastnosti okenního køídla - køídlo1
  IFCDOORSTYLE "Ingresso a 1 Anta 12" | SINGLE_SWING_LEFT | 1 occurrence | property sets: Vlastnosti èar dveøí, Vlastnosti dveøního panelu - panel1
  IFCSLABTYPE "Retino vuoto 3157531607 150" | FLOOR | 1 occurrence
  IFCWALLTYPE "Cartongesso 110 0598480581 100" | 13 occurrences
  IFCSLABTYPE "Minimal space 2632848274 220" | FLOOR | 1 occurrence
  IFCWALLTYPE "stena 3 0598480581 170" | 1 occurrence
  IFCWINDOWSTYLE "Okno 18" | SINGLE_PANEL | 1 occurrence | property sets: Vlastnosti èar okna, Vlastnosti okenního køídla - køídlo1
  IFCWINDOWSTYLE "2 Ante 12" | SINGLE_PANEL | 1 occurrence | property sets: Vlastnosti èar okna, Vlastnosti okenního køídla - køídlo1
  IFCSLABTYPE "Minimal space 2632848274 250" | FLOOR | 1 occurrence
  IFCWINDOWSTYLE "Dvoukøídlé okno 1 18" | DOUBLE_PANEL_VERTICAL | 1 occurrence | property sets: Vlastnosti èar okna, Vlastnosti okenního køídla - køídlo1, Vlastnosti okenního køídla - køídlo2
  IFCDOORSTYLE "1A 12" | SINGLE_SWING_LEFT | 3 occurrences | property sets: Vlastnosti èar dveøí, Vlastnosti dveøního panelu - panel1
  IFCDOORSTYLE "1A Scorrevole Esterna 12" | SLIDING_TO_RIGHT | 1 occurrence | property sets: Vlastnosti èar dveøí, Vlastnosti dveøního panelu - panel1
  IFCDOORSTYLE "1A 12" | SINGLE_SWING_RIGHT | 1 occurrence | property sets: Vlastnosti èar dveøí, Vlastnosti dveøního panelu - panel1
  IFCSLABTYPE "Muratura 1695224766 250" | ROOF | 2 occurrences

Property sets
  AC_Pset_RenovationAndPhasing | properties | on 35 objects (18 IFCWALLSTANDARDCASE, 6 IFCDOOR, 6 IFCWINDOW, 5 IFCSLAB)
    Renovation Status = "Existing" (IFCLABEL)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.0396 (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.9476 (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.3956 (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 2.8371 (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_FireRatingProperties | properties | on 12 objects (6 IFCDOOR, 6 IFCWINDOW)
    FireResistanceRating = "" (IFCLABEL)
  Pset_ManufacturerOccurrence | properties | on 5 objects (5 IFCWINDOW)
    SerialNumber = "" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 5 objects (5 IFCWINDOW)
    Manufacturer = "" (IFCLABEL)
    ProductionYear = "" (IFCLABEL)
  Pset_DoorCommon | properties | on 6 objects (6 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
  Vlastnosti èar okna | predefined | on 5 type objects
  Vlastnosti okenního køídla - køídlo1 | predefined | on 5 type objects
  Vlastnosti èar dveøí | predefined | on 4 type objects
  Vlastnosti dveøního panelu - panel1 | predefined | on 4 type objects
  Vlastnosti okenního køídla - køídlo2 | predefined | on 1 type object